BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0102
Traffic group

The command states which traffic group the extension belongs to at speech calls.

The traffic group controls which trunk lines and other extensions the extension can be connected to.

Extensions (and trunk lines) can be divided into 16 different traffic groups:

0 = Completely open

1-15 = Control according to the traffic group matrix

For data extensions command group 0139 Filter coefficient is used to determine an extension's traffic group.

The traffic group matrix specifies which traffic groups are permitted to be connected to each other. It is possible to open one traffic direction, e.g. outgoing, and to bar the opposite, incoming. The traffic group matrix is common for both voice and data calls.

##### Valid data: 0 (default)-15

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003