BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x6D
VMU Memory Error

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | VM |
Category: |  | MAINTENANCE |

An error has been found in the data in the VMU memory. This can be a program or a battery malfunction.

- D1:
- D2: Card position
- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003