BusinessPhone Communication Platform 5.1
Commands > Commands 5000...5999

## 5629
Pickup code for common bell

Common bell is a facility that permits all extensions to pick up the call from one defined common bell extension.

It is not possible to pick up the call from an operator or if the connection is prohibited by traffic group.

Here you can change the code for calling the feature PICK UP COMMON BELL EXTENSION

The code can have a length of max. 4 characters.

Valid characters:

0, 1, ...9

*, #

C, D, E

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: C © Ericsson Enterprise 2003