BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0xCB
Wrong Basic Access Mode

Default definition: |  | ERROR |
Used by block: |  | TR |
Category: |  | MAINTENANCE |

The programming of an ISDN S-/T‑interface was not accepted, because the selected connection mode does not correspond to the reported hardware interface.

- D1: Card position
- D2: Individual number
- D3: Undefined
- D4: Undefined

#### Recommended action

Check the programmed ISDN interface mode (command 1929) and/or the selection of the ISDN interface on the BTU-B DIP-switch.

Revision: PH2 © Ericsson Enterprise 2003