BusinessPhone Communication Platform 5.1
Commands > Commands 9000...9999

## 9146
Subscriber called party NL 4

91 x 6 SUBSCRIBER called party number length (S-NL) This command states the amount of digits in the SUBSCRIBER number part in case of proprietary CN calls. It is used to separate the SUBSCRIBER and DIALLED parts from a complete called party number.

Value = 1-20

not programmed = blank (no seaparation of called number)

The complete called party number length (C-NL) is defined in command 91 x 5.

For proprietary CN calls the complete called party number can be separated into a ‘SUBSCRIBER number part’ and a ‘DIALLED number part’: The length of the SUBSCRIBER number part (S-NL) is used to identify the called subscriber, i.e to reach a CN PBX. This number part is the most significant number part of a complete number. The ‘DIALLED number part’ will be the least significant number part of a complete number. This number part will be transferred as proprietary information via UUS 1 and it is used for continued addressing within the reached CN PBX.

e.g.: At CN VPN call a private network number is translated to corresponding public number and thereafter separated as:

C-NL = |  | 13 |  | 0222 81100 |  | 4701 |  | (COMPLETE called party number) |
S-NL = |  | 9 |  | 0222 81100 |  |  |  | (SUBSCRIBER number part) |
|  |  |  |  |  | 4701 |  | (DIALLED number part) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003