BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3821
Operator’s identity number for active

This command is used to state whether the ACD-operator must specify her/his identity on being marked active. The identity is used to faciliate identification of the ACD-operator for advanced traffic statistics using a PC.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003