BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0156
Direct diversion at external
calls?

If incoming external calls should be diverted, command 0156 must be programmed.

Note

Valid only for DID-calls. E.g.: Transferring an external call to an extension, which has activated “direct diversion for incoming external calls”, will NOT be affected via this command.

##### Valid data: Yes /No (default)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003