BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4324
OCN user acknowledgement time

This command specifies the time between the connection setup and the first key press. If this time passes without any user interaction, means that this was an unsuccessfull notification.

When a notification call takes place it is importat for the user to press a key. In this case the system will know that there is a real person on the other side and not a answering machine or and other mailbox system.

Valid values: |  | 1 - 255 sec. |
Default value: |  | 60 sec. |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003