BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 22 CONINFO

00h CONI.REAACT |  | Reanswer function activated |
01h CONI.REAREL |  | Release during activated reanswer |
02h CONI.REANSW |  | Reanswer during activated reanswer |
03h CONI.KEYREQ |  | Request of one key from the originator |
04h CONI.CALLPROG |  | Call progress info, from external party |
05h CONI.KEYRES |  | Trunk must reset the key buffer |
06h CONI.CNDIV |  | Diversion was executed in another CN PBX |
07h CONI.CNDNR |  | Diversion info was forwarded to term. PBX |
08h CONI.CNSOR |  | Signal to term. to initiate ringing |
09h CONI.CNTFR |  | New connected private identity |
0Ah CONI.ANUM |  | Calling party number |
0Bh CONI.FREL |  | A-party requests forced release of C-party |
0Ch CONI.ACDTFR |  | CONINFO ACD transfer |
0Dh CONI.BUSY |  | Call queued because of busy destination |
0Eh CONI.REGREQ |  | Request DTMF register |
0Fh CONI.REGACK |  | Register positive acknowledge |
10h CONI.REGNAK |  | Register negative acknowledge |
11h CONI.REGREL |  | Register release |
12h CONI.RELREQ |  | Release request from connected party |

Revision: PD2 © Ericsson Enterprise 2003