BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2072
MD110 release version of CN

This command is used to define the release of MD110 systems connected to the private network.

This is necessary because of enhacements and changes in MD110 proprietary UUS signalling protocol for digital networking features.

All nodes within the private network must be configured to the same release version!

#### Note for versions of BC10:

- BC10/1: released version of MD110
- BC10/2: released follow-up version of MD110 which includes the changed message layout for CN-call diversion and rerouting: B-party (diverting number) and C-party (diverted-to number) are exchanged in the messages.

Value: BC 8, BC 9, BC 10/1, BC 10/2

Initial value = BC 10/1

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003