BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0165
Diversion on no reply to slave?

The command defines whether or not a diversion on no reply to an associated slave extension should be done. If the extension is a master and a member of a tandem configuration the command data shall be copied to the slave and blocked for the slave’s further use.

##### Valid data: Yes (default) /No

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003