BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1103
Reroute position at day

This command is used to determine the rerouting position of the trunk in a day-switched exchange. To this position unanswered external calls i.e. parked calls, camped-on calls and transfer before answering are routed.

The rerouting position is determined by stating its directory number. The individual extension is removed by blanking out the current directory number.

If there is no rerouting position, the trunk will be parked for general access. The call will also be presented on all system telephones on which the trunk is represented by a function key.

The rerouting position is selected by stating its directory number. Erasure of the directory number results in erasure of the rerouting position.

The call will be presented on those system telephones where the trunk is represented by a key.

Note

If the individual answering position and the rerouting position are removed for the trunk, make sure that the trunk is represented on a function key so that incoming calls can be presented.

Therefore, please check commands 1101 Answering position at day, 1407 Maximum hold time and command group 03.

Valid values: 0-4 characters (0-9,*,#)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003