BusinessPhone Communication Platform 5.1
Dialogs

## Active Alarm / Heartbeat

The alarm function is used to send an alarm initiated by a telephone or an external alarm device to a pre-programmed alarm center. The Active Alarm / Heartbeat dialog consists of three sections:

- Identity
- Active Alarm
- Heartbeat

For further information about the alarm feature, please refer to the facility description of the Alarm Function (110/15534-ASB 150 02 Uen).

### Alarm settings:

- In the directory tree on the left side, click on the “+” in front of the “Features” menu. This will open the submenus.
- Click on the “Active Alarm / Heartbeat” submenu to open the Active Alarm / Heartbeat dialog.
- Define the alarm details.

- For a detailed information about a field, a setting, a check box or a drop-down list box, click on the command link in brackets. This will open an online help window for the selected command.
- For example, if you want to know more about the Service Area ID, click on the command link [7420] to view the command’s details.

- If you are satisfied with your changes, click on the Submit button to transfer your settings to the system. After your settings have been transferred to the system, the Active Alarm / Heartbeat dialog is displayed.

- or

- Click on the Reload button to discard all changes and entered values. The Active Alarm / Heartbeat dialog is set to default.

### Identity

7420 |  | Service area id

7421 |  | Identity of exchange

### Active Alarm

7430 |  | Active alarm on?

7431 |  | Active alarm I/O port

7432 |  | Active alarm receiver

7433 |  | Active alarm via internal modem

7434 |  | Active alarm number

7435 |  | Active pause number

7436 |  | Active alarm attempts

7437 |  | Max active alarms per day

### Heartbeat

7440 |  | Heartbeat on?

7441 |  | Heartbeat I/O port

7442 |  | Heartbeat receiver

7443 |  | Heartbeat via internal modem

7444 |  | Heartbeat number

7445 |  | Heartbeat pause

7446 |  | Heartbeat attempts

7447 |  | Heartbeat pace

#### Actions

Submit |  | To submit your settings to the system. |
Reload |  | To load the current system settings and to discard all entered data or changes. |

Revision: B © Ericsson Enterprise 2003