BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8410
Destination number modification

This command will be used to get the destination number (B-number) which should be sent to the carrier network and the corresponding external access code to be used.

In some cases it is necessary to delete leading digits from the public destination number. In other cases it is not necessary to modify the public number to get the B-number (they are equal).

Destination number:

The destination number (up to 10 digits) which should be modified.

Delete:

The number of digits (up to 10 digits from the very left position) of the destination number to be deleted to convert it to a carrier access code.

Carrier access code:

The carrier access code (up to 10 digits) which is inserted into the rest of the destination number in the leftmost position.

See command 8405 Detecting carrier access codes.

Example:

A carrier offers only international destinations. All international destinations start with 00. The external access code to be used to get access to the carrier network is specified as 190. The carrier has further specified that the two leading digits (00) need not be dialled.

Destination number |  | Delete Carrier |  | Access Code |
00 |  | 2 |  | 190 |

Note

If no destination number but a delete parameter or an access code is specified, this entry is valid for all destination numbers except those specified in the table.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003