BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## D4 ARCTRL

Control Automatic Redial feature.

00h AR.ACTIVATE | Request Automatic Redialling |
01h AR.RSPACTIVATE | Response to Automatic Redial request |
02h AR.CANCEL | Cancel Automatic Redialling |
03h AR.RSPCANCEL | Response to Automatic Redial cancelling |
04h AR.SUSPEND | Pause Automatic Redialling |
05h AR.RSPSUSPEND | Response to Automatic Redial pausing |
06h AR.RESUME | End pausing of Automatic Redialling |
07h AR.RSPRESUME | Response to Automatic Redial end pausing |
08h AR.READY | EX/OP idle indication |
09h AR.RESERVE | Reserve EX/OP instrument when AR is started |
0Ah AR.RSPRESERVE | Response to EX/OP instrument reserving |
0Bh AR.INVOKE | Make EX/OP to start call back ringing and to display 'Auto Redial Call' |
0Ch AR.SEIZBOOK | Make EX/OP to reroute own connection to AR to external party |
0Dh AR.RELEASE | Release EX/OP connections to AR |
0Eh AR.KEYINFO | Send programmable AR key data to AR |
0Fh AR.NUMBER | Send number to be redialled to EX/OP |

Revision: PD2 © Ericsson Enterprise 2003