BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0116
Hot line destination

The command states whether the extension is a so-called non-dialled connection extension, i.e. connection is achieved without dialling when the extension starts a call by lifting the handset or by pressing the ON/OFF key.

The non-dialled connection facility is activated by giving a 1-4 digit number.

The non-dialled connection facility is deactivated by over-writing the number with blanks.

System telephones with a line key can make calls as desired even if they are non-dialled connection extensions, by pressing a line key to initiate the call.

##### Valid data: 1-4 digit directory number

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003