BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1017
Reroute on incomplete number?

The command is used for direct in-dialing and private trunks for rerouting incoming calls to the rerouting position, if an inadequate number of digits has been received from a superior exchange. For rerouting to take place it is necessary that the rerouting position has been programmed, see commands 1103 Reroute position at day and 1104 Reroute position at night.

Valid values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003