BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4601
Record messages allowed ?

Voice messages, voice information and voice answers are stored on “voice memory boards”, VMU.

This command determines whether voice messages may be recorded on the stated board.

Valid Values: YES / NO

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003