BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2163
Signaling protocol

Defines the signalling protocol to be used towards the node defined by command 2164

##### Valid data

0 |  | None (default) |
1 - 100 |  | Reserved |
101 |  | ASB150 02 IP Gateway |
102-255 |  | Reserved |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003