BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3823
Voice message to operator

This command is used to state whether the ACD-operator shall be able to monitor the voice message on answer that has been programmed by command 3903 Voice message on answer.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003