BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2641
Alternative busy tone

The alternative busy tone is used because some external units, e.g. voice mail, cannot interpret the normal tone. See command 0125 Voice mail extension?. In this case, the alternative busy tone replaces the busy tone. The tone indicates that the called party is busy. The call will not be presented.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003