BusinessPhone Communication Platform 5.1
Start of Operation BP Management Suite

## Connection principles

Single installation means that BusinessPhone is connected to a standalone PC e.g. a laptop.

There are two options:

- Direct serial: BusinessPhone is connected directly via a V.24 cable to a standalone PC.
- Direct modem: BusinessPhone is connected via a standard modem to a standalone PC.

Network installation means that the BMS is installed within a LAN network. Several BusinessPhones are connected to PCs positioned somewhere in the network. The connection between the BMS and BusinessPhone will be established via the BMS Remote v.24 Agent.

- Remote serial: BusinessPhone is connected via V.24 to a PC on which the BMS Remote v.24 Agent is installed and from the BMS Remote v.24 Agent via LAN (TCP/IP) to the BMS.
- Remote modem: BusinessPhone is connected via Modem to a PC on which the BMS Remote v.24 Agent is installed and from the BMS Remote v.24 Agent via LAN (TCP/IP) to the BMS.
- IPU (TCP): BusinessPhone is connected via direct LAN connection to a PC and via LAN (TCP/IP) to the BMS.

Below the connection from the user interface (GUI) to BusinessPhone is illustrated:

### Standalone configuration

### Network configuration (via v.24 agent)

### Network configuration (IPU (TCP) connection)

### O&M from remotely connected computer

You can connect a PC with an BMS installation to the system remotely. There are two ways for remote connection:

with the PBX's built-in V.32bis modem:

via the Internet

Revision: B © Ericsson Enterprise 2003