BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4101
Operator line position

This command is used to state the position of those extension positions to which an operator is to be connected.

The line position is entered as: ppiii

where

pp = board position (00-63) |  |

iii = individual (000-107) of the operator extension |  |

A maximum of three operators are permitted.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003