BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3508
Flexible display

This command defines the type of display layout, which will be used by the called PBX group members during ringing.

Note

The flexible display will only be available on extensions, operators will not support this facility.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003