BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1022
Voice info to trunk allowed?

The command is used to state whether voice information for incoming trunk traffic shall be given to an extension possessing the voice information function.

Valid values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003