BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0502
Notification method

This command specifies which user has access to the outcall notification.

A user can activate his/her notification with this command when it is enabled.

This following table shows the possible settings to allow a user the outcall notification.

Valid data:
0 |  | Function disabled |
1 |  | Full notification |
2 |  | Brief notification |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003