BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## A8 TRTRANSIT

00H TRSEOSF |  | End of selection, free |
01H TRSEOSB |  | End of selection, busy |
02H TRSENDS |  | End signal |
10h TRSSUBS |  | Calling party is a subscriber |
11h TRSOPER |  | Calling party is an operator |
12h TRSADIG |  | A-number digit |
13h TRSAEND |  | End of A-number |
14h TRSAREJ |  | Request of A-number rejected |
15h TRSEXTDIV |  | External diverted call |
20h TRSACAT |  | Request of A-category |
21h TRSADDCMP |  | Complete address |
22h TRSBAR |  | Congestion or barred number |
23h TRSBUSY |  | Called party busy |
24h TRSCONG |  | Congestion before complete address |
25h TRSFREE |  | Called party free |
26h TRSSETUP |  | No result available, setup speech |
27h TRSUNALLO |  | Unallocated number |
28h TRSNXTDIG |  | Transfer of next digit |
29h TRSREQANO |  | A-number request |
2Ah TRSREQCLL |  | A-number request to incoming conn. TRUNK |
2Bh TRSREQGRA |  | A-group digits of B-number request to incoming conn. TRUNK |
2Ch TRSREQGRC |  | C-group digits of B-number request to incoming conn. TRUNK |
2Dh TRSREQALL |  | All digits of B-number request to incoming conn. TRUNK |
2Eh TRSSUBREJ |  | Request of A-category rejected |
2Fh TRSLINEOUT |  | Line-out before complete address |
40h TRSIRELEASE |  | ISDN trunk has been released |
41h TRSIFREE |  | ISDN trunk is released and free |
42h TRSIPROGRESS |  | Informs opposite ISDN party that ISDN trunk received SISIG,SIPROGRESS (with transparent data) |
45h TRSIFDATA |  | Transparent transfer of ISDN data between two TR parties i->o |
46h TRSIFDATAEND |  | o->i ended |
47h TRSIBDATA |  | i->o |
48h TRSIBDATAEND |  | o->i ended |
49h TRSISETUP |  | Sends SISETUP data to opposite trunk |
4Ah TRSICNSETUP |  | Sends SICNSETUP data to opposite trunk |
4Bh TRSIUUISETUP |  | Sends SIUISETUP to opposite trunk |
4Ch TRSISEIZACK |  | Seizure acknowledge from FW on outgoing side |
4Dh TRSICNALERT |  | Sends SICNALERT data to opposite trunk |
4Eh TRSIUUIALERT |  | Sends SIUUIALERT data to opposite trunk |
4Fh TRSIADDUUIALERT |  | Sends SIUUIBANSWER data to opposite trunk |
50h TRSISPEECH |  | Sends SIBANSWER data to opposite trunk |
51h TRSICNSPEECH |  | Sends SICNBANSWER to opposite trunk |
52h TRSIUUISPEECH |  | Sends SIUUIBANSWER to opposite trunk |
53h TRSICNDISC |  | Sends SICNDISC data to opposite trunk |
54h TRSIUUIDISC |  | Sends SIUUIDISC data to opposite trunk |
55h TRSIUUI |  | Sends SIUUIIN data to opposite trunk |
56h TRSIADDUUI |  | Sends SIADDUUIIN data to opposite trunk |
57h TRSIFACILITY |  | Sends SIFACILITY data to opposite trunk |
58h TRSIUUISERVICE |  | Sends SIUUISERVICE data to opposite trunk |
59h TRSIVIRSEIZACK |  | Seizure acknowledge from FW on outgoing side |
70h TRSIRGSDIGIT |  | Sends data received in SIRGSDIGIT to opp. trunk |
B4h TRSLOCSPEECH |  | MFC transit, call category: local speech |
B5h TRSLOCDATA |  | MFC transit, call category: local data |
B6h TRSSEMIAUTO |  | MFC transit, call category: semi automatic |
B7h TRSTOLLCALL |  | MFC transit, call category: toll automatic |
B8h TRSTESTCALL |  | MFC transit, call category: test |

Revision: PD2 © Ericsson Enterprise 2003