BusinessPhone Communication Platform 5.1
Commands > Commands 5000...5999

## 5209
Number of recall attempts

This command indicates the number of recall attempts to be made if the receiving device does not respond. Value 0-5.

Recall is a procedure in which an incoming call is not given direct access to the system. Instead, the call is terminated, after which the PABX makes an outgoing call to a predetermined number. This number is optional and should represent a party which is authorized for system access.

Commands 5208 Recall control-5211 Recall number concern the recall function.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: C © Ericsson Enterprise 2003