BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2080
Free second access

This command defines whether the system should by default work with the feature ‘Busy line 2’ (Yes) or with the feature ‘Free 2nd access’ (No). ‘Busy line 2’ means that every system telephone has by default two open lines for incoming calls whereby with ‘Free 2nd access’ there is only one. A key may be programmed to open/close the 2nd line.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003