BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8014
Wake-up answer anno 3

For a wake-up call to a guest a wake-up message can be supplied in the form of a voice message.

Wake-up messages can be given in three different languages.

With commands 8009 Wake-up language 1-8011 Wake-up language 3 the three languages in which wake-up-messages can be given are stated. Commands 8012 Wake-up answer anno 1-8014 Wake-up answer anno 3 are used to determine which wake-up messages shall be supplied for the respective language.

This command is used to determine the wake-up message to be supplied for the 1st language. This is done by stating a voice answer number for the voice message that has been recorded.

The voice answer number is created with command 5408 Create voice answer. Command 4701 Reference number for voice answer is used to determine the voice message references to be assigned to the number.

The references are recorded with a system telephone in system programming mode (See command group 4400).

Valid values: Directory number (initial value=no value)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003