BusinessPhone Communication Platform 5.1
Dialogs

## Tone Definition (repetitive)

Some tones are played in a loop. In this case the start point can be given.

Command | Value
Internal fragment | Value Range: 0-19 (15)
External fragment | Value Range: 0-19 (15)
Signal Time | Value Range: 0-16000 s (empty means continuous)
Pause time | Value Range: 0-16000 s (empty means continuous)
Start repetition here | Marks the element which starts the loop.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |

See facility description Ring And Tone Signals (443/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003