BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6007
Character set

The command defines which set of characters shall apply for the local-connected unit for the stated I/O-port .

0 = The PABX's internal set of characters (no characters are converted) |  |

1 = US-ASCII |  |

2 = Swedish/Finnish ASCII |  |

3 = Character set 2 in printer ERICSSON 7111 (strapped for compatibility with IBM-PC) and character set 850 (Multilingual) for SOFTECH hotel computer |  |

4 = Danish/Norwegian ASCII |  |

5-9 = Undefined values |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003