BusinessPhone Communication Platform 5.1
Commands > Commands 5000...5999

## 5413
Create common abbreviated number series

ASB 150 features a service called 'common abbreviated numbers'. On a call to a common abbreviated number, the abbreviated number is translated into a new number containing up to 17 digits.

Each common abbreviated number corresponds to a directory number in the system. This command is used for creating a directory number series for abbreviated numbers. Up to 16 such number series can be created. The abbreviated numbers can be allocated any directory number series, provided the series is vacant and does not conflict with existing directory numbers.

The - character is used as “wild card” when defining the directory number series.

Example:

Directory number series | Defined abbreviated numbers
602 | 602
61- | 610-619
62-- | 6200-6299
5--- | 5000-5999

Valid values: 4 digits (0-9,*,#)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: C © Ericsson Enterprise 2003