BusinessPhone Communication Platform 5.1
Commands > Commands 7000...7999

## 7433
Active alarm via int modem?

The command determines whether active alarms are to be sent via a built-in modem.

‘Active alarm’ is a function which transfers alarms to an external alarm receiver.

Commands 7420 Service area id, 7421 Identity of exchange and 7430 Active alarm on?-7437 Max active alarms per day concern active alarms.

Valid values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003