BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4006
Queue announcement time

A voice message can be supplied to external incoming calls that are in the PBX-operator queue.

This command is used to state after which time the voice message shall be supplied.

Range of values = 0-255 s

If the time is set to 0, no voice message will be supplied.

It is required that the reference number used has been programmed in accordance with commands 4007 Queue announcement reference and 4401 Voice Announcements.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003