BusinessPhone Communication Platform 5.1
Commands > Commands 9000...9999

## 9104
Call class

The command is used to define the type of ‘call class’ for some market specific traffic cases.

In case of Spanish market the external CN (VPN) call setup for this call destination can be defined as an IBERCOM call with related parameters.

The used network protocol on the actual (-T) link must be set to ‘network acc. to Spain’. This command overrides the corresponding trunk command (1036 Type of IBERCOM netw. conn.).

Value: not specified (non IBERCOM call) interuser IBERCOM call intrauser IBERCOM call

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003