BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x49
Buffer Error

Default definition: |  | ERROR |
Used by block: |  | RP |
Category: |  | DESIGNER |

Buffer error.Some errors have been found. The meaning of D2 depends on the value of D1.

D1 | Type of buffer error | D2 | Additionl data
00h | Trying to use a released buffer |  | Block ID (ST)
01h | Trying to send a released buffer |  | Block ID (ST)
02h | Number of free buffers below limit |  | 0
03h | Number of buffers out of control from OS below limit |  | 0

Some special definitions have been introduced for the CPU-D4 central processor board.

D1 | Type of buffer error | D2 | Additionl data
00h | Work buffer troubles |  | V.24 port number
01h | Work buffer troubles |  | V.24 port number
02h | Work buffer troubles |  | V.24 port number
04h | Signal buffer watermark |  | V.24 port number
05h | Signal buffer watermark |  | V.24 port number
06h | Signal buffer watermark |  | V.24 port number
07h | Signal buffer watermark |  | V.24 port number
08h | Signal buffer watermark |  | V.24 port number

- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003