BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6420
Flexible CIL- format

This command is used to create the personal call information loggigng record. All available CIL - data information are in a pool which could be selected to configure the own CIL - record.

This command covers a configuration table, containing all available data fields with their number of characters.

No. | CIL-Data Information | Character
1 | Message code | (2)
2 | Sequence number CIL4 | (3)
3 | Call date CIL4 | (6)
4 | End time CIL4 | (4)
5 | Caller´s number CIL4 | (4)
6 | Call duration CIL4 | (5)
7 | Meter pulses CIL4 | (4)
8 | Dialled access code CIL4 | (4)
9 | Dialled number CIL4 | (24)
10 | Information status 2 CIL4 | (1)
11 | Account code CIL4 | (15)
12 | Authorisation code CIL4 | (4)
13 | Queue time, answer CIL4 | (4)
14 | Information status 1 CIL4 | (1)
15 | Cost CIL4 | (11)
16 | Cost state CIL4 | (1)
17 | Trunk number CIL4 | (4)
18 | Sent access code CIL4 | (4)
19 | Sent number CIL4 | (24)
20 | A-number CIL4 | (20)
21 | Call via facility CIL4 | (1)
22 | Transfer condition CIL4 | (2)
23 | Carriage return/LF | (2)
24 | Sequence number + A HIS | (4)
25 | Hotel ALPHA HIS | (3)
26 | Call date (mmdd) HIS | (4)
27 | Caller´s number HIS | (5)
28 | End time (hhmm) HIS | (4)
29 | Call duration (minutes) HIS | (4)
30 | Called number HIS | (14)
31 | Hotel ALPHA EBC | (3)
32 | Call duration (hhmm/10) ASB | (4)
33 | Information status ASB | (1)
34 | Called number ASB | (20)
35 | Caller´s number DDI | (8)
36 | Space 1....(place reservation) | (1)^
37 | Space 5....(place reservation) | (5)
38 | Space 10...(place reservation) | (10)
39 | End time hh:mm:ss | (8)
40 | TAG identifier | (5)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003