BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0168
Use ACD key layout

The command defines whether or not the ACD key layout shall be used on a DBC 2x1/2x2 telephone.

Valid data:
0 |  | business layout |
1 |  | ACD key layout with clerical key |
2 |  | ACD key layout without clerical key |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003