BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2640
Alternative ring tone

The alternative ringing tone is used because some external units, e.g. voice mail, cannot interpret the normal tone. See command 0125 Voice mail extension?. In this case, the alternative ringing tone replaces ringing tone, special ringing tone or queue tone. The tone indicates that the call is presented at the called party.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003