BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0x93
First E2 Read/Write Failed

Default definition: |  | ERROR |
Used by block: |  | OM |
Category: |  | DESIGNER |

A write to the E2 area has failed at the first attempt. Timeout or E2NAK has been received. A second attempt will be made in most cases.

- D1:
- D2: Map number of E2 memory
- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003