BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0124
Call waiting tone for analogue extensions?

This command states whether or not the extension is allowed to receive a call-waiting tone.

Only analogue extensions are concerned, as digital extensions use the tone-ringer to announce call waiting. In this respect cordless telephones connected via a digital extension board are regarded as analogue.

##### Valid data: Yes / No (default)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003