BusinessPhone Communication Platform 5.1
Commands > Commands 6000...6999

## 6502
Listing of data for directory numbers

A printout of the programmed dataposts is done. The assignment of a namestring to a non guest directory number is done with the command 6501.

A datapost for guests is prepared by doing a check in (by hotel function key * 31 #).

##### Three types of printout can be ordered:

ALL Dataposts for guest and non guest extensions are printed. |  |

GUEST Dataposts for guest extensions are printed. |  |

DIR Dataposts for all non guest extensions are printed. |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2003