BusinessPhone Communication Platform 5.1
Dialogs

## Packet Mode Communication Statistics

This dialog shows the statistics of the packet mode communication.

The read-out statistics is useful for detecting simpler faults.

When a Packet Mode Communication Link is removed, only the State field is changed. The “Interface Number” and TEI fields are initialized, when a Packet Mode Communication Link is set-up. The “Transmitted” and “Discard I-Frame” fields are cleared, when a Packet Mode Communication Link is set-up.

| Value
Card | Shows all available cards in the system.
PMC | Packet Mode Communication Link
Interface number | Physical interface number on board. 0 - 7 = Valid values for BTU-B 0 - 3 = Valid values for MFU or sub-equipped BTU-B
TEI | Terminal Endpoint Identifier value in use for this data-link. 0 - 63 = TEI values in the non-automatic range are only valid.
State | Shows the state of the data link. 0 = Unassigned. No TEI value exists. Packet mode communication link is not established. 4 = TEI assigned. TEI value exists but the data link is not established. 5 = Awaiting establish. Waiting for acknowledge from peer. 6 = Awaiting release. Waiting for acknowledge from peer. 7 = Established. Frames can be send and received. 8 = Time-out state
Transmitted I-Frames | The number of transmitted I-Frames on this data-link to it is peer
Discard I-Frames | The number of frames that could not be forwarded from A-side to B-side or vice versa

#### Actions

Submit |  | To submit your changes to the system. |

Revision: B © Ericsson Enterprise 2003