BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2172
Gatekeeper identifier

In order to distinguish between the different installed Gatekeepers on the customer’s LAN, this command is used to define a unique name (identifier) for each Gatekeeper (according to ITU-T Recommendation H.323.)

The identifier is used for IP-clients which are sending out a multicast gatekeeper request to search for a gatekeeper with a specific name. The identifier is not needed, if the IP-clients are sending out a unicast gatekeeper request to a specific IP-address.

Note

As we don’t support multicast gatekeeper requests in ASB 150 02 R13, this command does not need to be set.

##### Valid data

0-35 |  | characters |
empty (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003