BusinessPhone Communication Platform 5.1
Commands > Commands 5000...5999

## 5208
Recall control

This command indicates whether recalls are to be made and, if so, for what types of call.

Recall is a procedure in which an incoming call is not given direct access to the system. Instead, the call is terminated, after which the PABX makes an outgoing call to a predetermined number. This number is optional and should represent a party which is authorized for system access.

0 = No recalls are allowed |  |

1 = A recall will be made only if the call was directed to a V.24 port |  |

2 = A recall will be made only if the call was directed to the directory number defined for system access |  |

3 = A recall will be made after all types of call, except those extended by an extension or the operator |  |

Commands 5208 Recall control-5211 Recall number define the recall procedure.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: C © Ericsson Enterprise 2003