BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0401
Available keys

This menu shows the individual abbreviated numbers for selected extension. Individual abbreviated numbers are stored via a programmable key. This command states which digits are to be included in the individual abbreviated number for the stated programmable key.

#### The following digit keys are allowed:

0-9 Digit to be sent

*,# Digit to be sent

- (wait for second dial tone)

space (erase the abbreviated number)

#### Individual abbreviated number dialling via the key pad

The procedures are related to the following keys:

**1 |  | key 05 |  | (= respective prog. key E) |
**2 |  | key 06 |  | (= respective prog. key F) |
**3 |  | key 07 |  | (= respective prog. key G) |
**4 |  | key 08 |  | (= respective prog. key H) |
**5 |  | key 09 |  | (= respective prog. key I) |
**6 |  | key 10 |  | (= respective prog. key J) |
**7 |  | key 11 |  | (= respective prog. key K) |
**8 |  | key 12 |  | (= respective prog. key L) |
**9 |  | key 13 |  | (= respective prog. key M) |
**0 |  | key 14 |  | (= respective prog. key N) |

##### Valid data: 1-24 digit number

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003