BusinessPhone Communication Platform 5.1
VMU-HD & MFU

## Title 8a: Mailbox System - Message Storing & Retrieving (Command 4428)

No. | Filename | Predefined texts
0 | D440D440.001 | Main Menu: To listen to your messages, press ONE, To change your greetings, press TWO, To exit, hang up
1 | D441D441.001 | Greetings: - to change your greeting, when the line is busy, press ONE, On no reply, press TWO, For direct diversion, press THREE To go back to the main menu, press Oh (0)
2 | D442D442.001 | To record your greeting, press ONE, To listen to it, press TWO, To delete it, press THREE, To go back to the greeting menu, press NINE, Or to go back to the main menu, press Oh (0)
3 | D443D443.001 | This feature is currently not available, please try again later..
4 | D444D444.001 | Recording time exceeded. Your greeting has not been recorded.
5 | D445D445.001 | No greeting recorded.
6 | D446D446.001 | Greeting recorded.
7 | D447D447.001 | Greeting deleted.
8 | D448D448.001 | End of messages - To return to message retrieval, press NINE, To go back to the main menu, press Oh(0) To exit, hang up.
9 | D449D449.001 | There is no previous message.
10 | D44AD44A.001 | Message Retrieval: - To listen to new messages, press ONE, To listen to messages already heard, press TWO, To lsiten to stored messages, press THREE.
11 | D44BD44B.0011 | (VOICE CONTROL - STANDARD MBX - FOR NEW MESSAGES ONLY - R13): To replay, press ONE, To send a copy to someone else, press TWO, For time stamp, press THREE, To pause or continue during replay, press FIVE, To store this message, press EIGHT, For the next message, press NINE, To delete this message, press HASH.
12 | D44CD44C.0012 | (VOICE CONTROL - STANDARD MBX - FOR STORED MESSAGES ONLY - R13): To replay, press ONE, To send a copy to someone else, press TWO, For time stamp, press THREE, To pause or continue during replay, press FIVE, For the previous message, press SEVEN, To store this message again, press EIGHT, For the next message, press NINE, To delete this message, press HASH.
13 | D44DD44D.001 | Message stored for ...
14 | D44ED44E.001 | ...days.
15 | D44FD44F.001 | Archive full. Please try again later.
16 | D450D450.001 | Your archive is full. To store this message, delete another stored message.
17 | D451D451.001 | After the tone, please record you greeting, - to finish recording, press HASH.
18 | D452D452.001 | End of messages. - For the last message, press SEVEN, To return to message retrieval, press NINE, To go back to the main menu, press Oh (0) To exit, hang up.
19 | D453D453.0013 | (VOICE CONTROL - STANDARD MBX - FOR HEARD MESSAGES ONLY - R13): To replay, press ONE, To send a copy to someone else, press TWO, For time stamp, press THREE, To pause or continue during replay, press FIVE, For the previous message, press SEVEN, To store this message, press EIGHT, For the next message, press NINE, To delete this message, press HASH.
20 | D454D454.001 | Main Menu:
21 | D455D455.001 | To listen to your messages, press ONE,
22 | D456D456.001 | To change your greetings, press TWO,
23 | D457D457.001 | To send a message, press THREE,
24 | D458D458.001 | To set up outcall notification, press FOUR,
25 | D459D459.001 | To change your password, press FIVE, To exit, hang up.
26 | D45AD45A.001 | End of messages. - To go back to the main menu, press Oh (0) To exit, hang up.

1 Old recordingname: 4429-3, R12 prompt. 2 Old recordingname: 4429-5, R12 prompt. 3 Old recordingname: 4429-4, R12 prompt. e.g. “Message stored for” - “Twenty” - “days” (4428-13 + 4405-x + 4428-14)

Revision: A © Ericsson Enterprise 2003