BusinessPhone Communication Platform 5.1
Commands > Commands 2000...2999

## 2341
Traffic check at operator conference

This command states how the traffic group check should be executed before an operator three-party connection is allowed.

Alternatives:

0 = It is only necessary that the operator is open to call or receive calls from all parties in the three-party connection. |  |

1 = The operator has to be open in relevant directions to all parties and there must be at least one direction open between the other two parties. |  |

2 = The traffic group has to be open in both directions between all parties in the three-party connection. |  |

3-9 Reserved. |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2003