BusinessPhone Communication Platform 5.1
Dialogs

## Trunk Route Delete

To delete a trunk route, click on the facility’s Delete link. BMS will display a delete dialog.

Note

You cannot delete trunk route 0, but you can change its directory number and name.

Select all facilities that you want to delete and press the Delete button. To abort the deletion process and return to the create/select/change dialog, press the Cancel button.

The Delete Trunk Routes dialog allows you to delete one route or even several trunk routes at the same time.

To access the dialog, open the “Trunks” menu in the Configuration directory tree and click on the “Trunk Routes” submenu. The Trunk Routes dialog is displayed. The Edit/Change Trunk Routes section shows a list of all available routes. Click on the Delete link of a route that you would like to delete.

### Deleting a trunk route:

- Click in the check box of one or more trunk rout(es) that you want to remove from the system.
- Click on the Delete button. All selected trunk routes are removed from the system. You will return to the Trunk Routes dialog automatically.

- or

- Click on Cancel to abort the process and to return to the Trunk Routes dialog without submitting any changes.

#### Actions

Delete |  | To delete the selected trunk route(s). |
Cancel |  | To abort the process. |

See also facility descriptions:

- Route Selection (444/15534-ASB 150 02 Uen).
- Trunk (486/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003